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ABSTRAK

Penelitian ini bertujuan untuk menentukan percepatan getaran tanah maksimum (PGA) dengan menggunakan metode Tong & Katayama (1988) kemudian divisualisasikan dengan mikrozonasi PGA, intensitas gempa dengan Persamaan Wald, dan indeks kerentanan seismik (Kg) kemudian divisualisasikan dengan mikrozonasiKg di Dusun Patuk.

Data penelitian diperoleh melalui pengukuran mikrotremor di 13 titik lokasi pengambilan data. Data mikrotremor kemudian dianalisis menggunakan metode Horizontal to Vertical Spectral Ratio (HVSR) untuk mendapatkan frekuensi predominan dan faktor amplifikasi di setiap titik penelitian. Hasil dari analisis mikrotremor digunakan untuk menentukan nilai indeks kerentanan seismik (Kg), nilai percepatan getaran tanah maksimum diperoleh dengan menggunakan metode Tong & Katayama (1988), dan nilai intensitas gempa diperoleh dari hasil percepatan getaran tanah maksimum.

Hasil studi ini menyatakan bahwa nilai percepatan getaran tanah maksimum di Dusun Patuk adalah 53,58 cm/s2 sampai 57,51 cm/s2 dengan intensitas gempa V MMI. Berdasarkan tingkat kerawanan gempa dalam skala intensitas gempabumi diperoleh hasil bahwa Dusun Patuk berada pada tingkat potensi gempabumi risiko tinggi untuk TA 13. Risiko sedang untuk TA 3, risiko ringan untuk TA 5. Kemudian untuk analisis indeks kerentanan seismik di Dusun Patuk diperoleh nilai yang berkisar antara 0,32 [image: image2.png]X 107®
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 s2/cm. Indeks kerentanan seismik terendah di Dusun Patuk berada di TA 9 dan tertinggi di TA 1.
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ABSTRACT

The aims of this study are to determine the peak ground acceleration (PGA) using Tong & Katayama (1988) method, then visualized with PGA microzonation, to determine the intensity of the earthquake using Wald Equation, and to determine the vulnerability index (Kg), then visualized with Kg microzonation in Patuk Village Gunung Kidul Regency.

Data were obtained by microtremor measurement at 13 locations. The microtremor data were analyzed using Horizontal to Vertical Spectral Ratio (HVSR) method to obtain the predominant frequency at each measurement point. The result of the microtremor analysis were used to determine the seismic vulnerability index (Kg), the peak ground acceleration values obtained using the method of Tong & Katayama (1988), and the intensity of the earthquake value from the peak ground acceleration.

The results show that the peak ground acceleration value in Patuk Village is between 53,58 cm/s2 to 57,51 cm/s2 with earthquake intensity V MMI (Modified Mercalli Intensity). Based on the seismic vulnerability of earthquake intensity scale, the results obtained show that Patuk Village is located at the high risk level of earthquake at TA 13. The moderate risk is at TA 3, and the low risk is at TA 5. Then, results of the seismic vulnerability index in Patuk Village is 0,14 [image: image6.png]X 107®
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 s2/cm. Seismic vulnerability index in Patuk Village is lowest at TA 9 and highest at TA 1.
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